# Sandsara Tracks and Firmware
## Firmware
- Introduce the new SD card into your computer.
- Download the new Firmware at your computer.
- It is essential to have the file individually, not a ZIP form.
- Paste Firmware directly into the SD card (the files mustn't be in any folder, just the files directly into the SD card)
- Insert the SD card in your Sandsara.
- Plug in your Sandsara.
## Format your SD Card with fat32

## Tracks and Firmware
Adding tracks and firmware to the Sandsara is pretty straightforward it's basically drag these files into the SD card fully unplug and fully plug in the sd card and do all the work with the Sandsara unplugged and then plug it back in when the SD is updated.

## Make sure your card is not counterfit.
Look for a windows SD/USB storage validation tool called [ValiDrive](https://www.grc.com/validrive.htm) there are a lot of drives that lie about their storage capacity on the chip level, convincing your computer that it's not writing data into oblivion this tool will ensure your SD card is valid and functional as described do not trust drives that fail this tool and do your best to report bad sources to the stores you bought them from or your local police.